Lynx

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  | **L2Audio (D25)** | | | |  |
|  | Pin | Signal | Pin | Signal |  |
|  | 1 | OUT4 Hot | 14 | OUT4 Cold |  |
|  | 2 | OUT4 Gnd | 15 | IN4 Hot |  |
|  | 3 | IN4 Cold | 16 | IN4 Gnd |  |
|  | 4 | OUT3 Hot | 17 | OUT3 Cold |  |
|  | 5 | OUT3 Gnd | 18 | IN3 Hot |  |
|  | 6 | IN3 Cold | 19 | IN3 Gnd |  |
|  | 7 | OUT2 Hot | 20 | OUT2 Cold |  |
|  | 8 | OUT2 Gnd | 21 | IN2 Hot |  |
|  | 9 | IN2 Cold | 22 | IN2 Gnd |  |
|  | 10 | OUT1 Hot | 23 | OUT1 Cold |  |
|  | 11 | OUT1Gnd | 24 | IN1 Hot |  |
|  | 12 | IN1 Cold | 25 | IN1 Gnd |  |
|  | 13 | none |  |  |  |
|  | The LynxTWO B Model replaces IN 3 and IN 4 with OUT 5 and OUT 6. | | | | |
|  | The LynxTWO C Model replaces OUT 3 and OUT 4 with IN 5 and IN 6. | | | | |

RME cable pinouts

